[header]
* Input parameters for MQLatency program *
*
*
* name of the queue and queue manager
* to write messages to
*
qname=LATENCY.IN
qmgr=WBRK6_QM
*
* total number of messages to be written
* the program will stop after this number of
* messages has been written
*
msgcount=25

*
* number of milliseconds to delay after getting each reply
*
sleeptime=20

*
* MQMD format field
*
format= "MQSTR   "
*
* Correlation id specified in ASCII
*
*correlid="Performance Utility Test  "
* 
* Correlation id specified in Hex
*
*correlidx=20313233343536000037381a1b1c00
*
* Message priority
*
priority=2
*
* group id specified in ASCII
*
*groupid=group 1  
*
* group id specified in hex
*
*groupidx=c1c2f1f2
*
* reply to Queue manager
*
replyqm=WBRK6_QM
*
* reply to queue name
*
replyq=LATENCY.REPLY
*
* message persistence
* persist no = 0
* persist yes = 1
* persist as queue def = 2
*
persist=0
*
* message type
*
* Allowed values for message type
*  1 - request
*  2 - reply
*  4 - report
*  8 - datagram
*  112 - MQE fields from MQE
*  113 - MQE fields
*  65536 to 999,999,999 - user
msgtype=1
* new message id for each message written
newmsgid=Y
* match on correlation id for reply messages
getbycorrelid=Y
*
* encoding for user data 
* encoding=273 for AIX integers, etc
* encoding=546 for PC integers, etc
* encoding=785 for host 390 integers, etc
*
encoding=546
*
* code page for user data
* codepage=437 for US PC characters (ASCII)
* codepage=500 for US host characters (EBCDIC)
*
codepage=437
*
* the character sequence that separates messages in a file 
*  message delimiter parameters in ascii or hex
* only one or the other should be specified
*
* delimiter="#$%^&"
* delimiterx="0D0A"
*
* rfh usage
* rfh = N for No rfh
* rfh = A for Automatic (look for RFH at beginning of data file)
* rfh = 1 or V1 for Version 1 rfh from parameters in parm file
* rfh = 2 or V2 for Version 2 rfh from parameters in parm file
* rfh = X for special V2 rfh with fixed portion only and format=xml
*
* only first character checked, except for V when second character is also checked
*
rfh=N
*
* rfh data parameters - only used if rfh=1 or rfh=2
*  ignored if rfh=N, rfh=A or rfh=X
*
* both V1 and V2
*  encoding should be 546 for PC and 785 for host 390
RFH_CCSID=500
RFH_ENCODING=785
* V2 only
RFH_NAME_CCSID=1208
RFH_DOMAIN=MRM
RFH_MSG_SET=DH4M6DO072001	
RFH_MSG_TYPE=Customer_Root
RFH_MSG_FMT=CWF
* V1 only
RFH_APP_GROUP=Customer_Msgs
RFH_FORMAT=Customer_Root
*
*
* END OF PARAMETERS SECTION
*
* beginning of list of message data files
* each line must contain a fully qualified file name
* each file will provide the data for a separate message
* the messages will be written in the order given below
* only file names may follow the [filelist] entry
*
[filelist]
* names of the data files
* can be fully or partially qualified
*
msg1.dat
*msg2.dat
*c:\v2test\rfhtest\msg3.dat